How to Update Mediacento IPX Firmware:

1. Connect to the web interface using the device’s IP address

2. Under the System tab (which should be selected by default) select “Update Firmware”

3. Browse and select for the desired firmware

4. Select Upload. This will cause the firmware to be installed and the device will reboot

5. Upon reboot the web interface will need to be reloaded