MediaCento Firmware Upload

To change the firmware on the MediaCento two things are needed:

1. IP address of the unit that will be upgraded

2. Firmware from FTP site

Process:

1. Connect to the MediaCento web interface with the IP address
2. Under System tab open Update Firmware
3. Select browse
4. Select the firmware file you wish to upload
	1. For receivers this will end in a “c” (ex: webfw**c**)
	2. For transmitters this will end in a “h” (ex: webfw**h**)
5. Select Upload

A few notes about uploading new firmware

* During firmware upload do not disconnect power or Ethernet connection
* IP address, netmask, and other settings will not change during upgrade
* Older versions are NOT compatible with the most recent firmware
	+ This means all units communicating will need to be consistent with firmware